bea.com | products | dev2dev | support | askBEA

Download Docs | Site Map | Glossary
Search

Administration Console Online Help

SNMP --> Traps --> Gauge Monitor --> General

Tasks Additional Documentation Attributes

Overview

Use this tab to configure Gauge Monitors.

Tasks

Configuring a Gauge Monitor

Additional Documentation

(Requires an Internet connection.)

WebLogic SNMP Management Guide

W ebLogic SNMP MIB Reference

Attributes

Attribute Label | Description | Value Constraints
--- | --- | ---
Name | The name of this configuration. WebLogic Server uses an MBean to implement and persist the configuration. MBean: weblogic.management. configuration. SNMPGaugeMonitorMBean Attribute: Name | Configurable: yes Readable: yes Writable: yes
Monitored MBean Type | Defines the type of the MBean to monitor. MBean: weblogic.management. configuration. SNMPGaugeMonitorMBean Attribute: MonitoredMBeanType | Configurable: yes Readable: yes Writable: yes
Monitored MBean Name | Defines the name of the MBean to monitor. MBean: weblogic.management. configuration. SNMPGaugeMonitorMBean Attribute: MonitoredMBeanName | Configurable: yes Readable: yes Writable: yes
Monitored Attribute Name | Defines the name of an attribute to monitor. MBean: weblogic.management. configuration. SNMPGaugeMonitorMBean Attribute: MonitoredAttributeName | Configurable: yes Readable: yes Writable: yes
Polling Interval | Defines the frequency the agent checks the attribute value. MBean: weblogic.management. configuration. SNMPGaugeMonitorMBean Attribute: PollingInterval | Units: seconds Minimum: 0 Maximum: 65535 Default: 0 Configurable: yes Readable: yes Writable: yes
Threshold High | Defines the high threshold at which a trap is generated. A trap is generated if the monitored value is equal to or greater than this value. MBean: weblogic.management. configuration. SNMPGaugeMonitorMBean Attribute: ThresholdHigh | Default: 0 Configurable: yes Readable: yes Writable: yes
Threshold Low | Defines the low threshold at which a trap is generated. A trap is generated if the monitored value is less than or equal to this value. MBean: weblogic.management. configuration. SNMPGaugeMonitorMBean Attribute: ThresholdLow | Default: 0 Configurable: yes Readable: yes Writable: yes