bea.com | products | dev2dev | support | askBEA

Download Docs | Site Map | Glossary
Search

Administration Console Online Help

Network Channel Fine Tuning --> Configuration --> General

Tasks Additional Documentation Attributes

Overview

Use this page to add a Listen Address to use with the network channel assigned to this server, or to override the Listen Port settings associated with the network channel.

Note that the changes you make to this page are reflected in a NetworkAccessPointMBean for the server, and do not affect the network channel properties of other servers or clusters that use the channel.

Values of -1 mean that the server uses the same Listen Port configuration as the network channel.

Tasks

Configuring a Network Access Point

Additional Documentation

(Requires an Internet connection.)

Network Access Points (NAPS)

Network Channels

Attributes

Attribute Label | Description | Value Constraints
--- | --- | ---
Listen Address | A value of null indicates that this value is inherited from the server. MBean: weblogic.management. configuration. NetworkAccessPointMBean Attribute: ListenAddress | Default: null Configurable: yes Readable: yes Writable: yes
Listen Port | The plaintext (non-SSL) listen port for the channel. -1 implies that this value is inherited from the channel. MBean: weblogic.management. configuration. NetworkAccessPointMBean Attribute: ListenPort | Default: -1 Configurable: yes Readable: yes Writable: yes
SSL Listen Port | The SSL listen port for the channel. -1 implies that this value is inherited from the channel. MBean: weblogic.management. configuration. NetworkAccessPointMBean Attribute: SSLListenPort | Default: -1 Configurable: yes Readable: yes Writable: yes