bea.com | products | dev2dev | support | askBEA

Download Docs | Site Map | Glossary
Search

Administration Console Online Help

Local WLS Domains --> General

Tasks Additional Documentation Attributes

Overview

Local WLS Domains provide a view of local domains as they appears to other (remote) domains. You must have at least one Local WLS Domain in a WTCServer configuration.

Tasks

Creating a Local WLS Domain

Additional Documentation

(Requires an Internet connection.)

Configuring WebLogic Tuxedo Connector

Attributes

Attribute Label | Description | Value Constraints
--- | --- | ---
Access Point | Defines a unique name within the scope of MBean types WTCLocalTuxDom and WTCRemoteTuxDom used to identify the access point or domain. MBean: weblogic.management. configuration. WTCLocalTuxDomMBean Attribute: AccessPoint | Readable: yes Writable: yes
Access Point Id | Defines the domain access point identifier. This identifier is a unique name across all local and remote domain access points. MBean: weblogic.management. configuration. WTCLocalTuxDomMBean Attribute: AccessPointId | Readable: yes Writable: yes
Network Address | Defines the network address of the local domain gateway. Specify the TCP/IP address in one of the following formats: //hostname:port_number //#.#.#.#:port_number If the hostname is used, the domain finds an address for hostname using the local name resolution facilities (usually DNS). If dotted decimal format is used, each # should be a number from 0 to 255. This dotted decimal number represents the IP address of the local machine. The port_number is the TCP port number at which the domain process listens for incoming requests. MBean: weblogic.management. configuration. WTCLocalTuxDomMBean Attribute: NWAddr | Readable: yes Writable: yes