bea.com | products | dev2dev | support | askBEA

Download Docs | Site Map | Glossary
Search

Administration Console Online Help

TUXEDO Queuing Bridge --> Priority Mapping

Tasks Additional Documentation Attributes

Overview

Use priorityMapping to map priorities between the JMS and Tuxedo. JMS has ten priorities (0 - 9); Tuxedo/Q has 100 priorities (1 - 100). There are two mapping directions: JmstoTux and TuxtoJms. Defaults are provided for all values, shown below in pairs of value:range.

JmstoTux- 0:1 | 1:12 | 2:23 | 3:34 | 4:45 | 5:56 | 6:67 | 7:78 | 8:89 | 9:100

TuxtoJms- 1-10:0 | 11-20:1 | 21-30:2 | 31-40:3 | 41-50:4| 51-60:5 | 61-70:6 | 71-80:7 | 81-90:8 | 91-100:9

Tasks

Configuring Priority Mapping for a tBridge Connection

Additional Documentation

(Requires an Internet connection.)

Configuring tBridge

Attributes

Attribute Label | Description | Value Constraints
--- | --- | ---
Jms To Tux Priority Map | Defines the mapping of priorities from JMS to Tuxedo. The are 10 possible JMS priorities(0=>9) which can be paired to 100 possible Tuxedo priorities(1=>100). A mapping consists of a "|" separated list of value-to-range pairs (jmsvalue:tuxrange) where pairs are separated by ":" and ranges are separated by "-". Examples 0:1 | 1:12 | 2:23 | 3:34 | 4:45 | 5:56 | 6:67 | 7:78 | 8:89 | 9:100 OR 0:1-10|1:11-20|2:21-30|3:31-40|4:41-50|5:51-60|6:61-70|7:71-80|8:81-90|9:91-100 MBean: weblogic.management. configuration. WTCtBridgeGlobalMBean Attribute: JmsToTuxPriorityMap | Readable: yes Writable: yes
Tux To Jms Priority Map | Defines the mapping of priorities to map from Tuxedo to JMS. The are 100 possible Tuxedo priorities(1=>100) which can be paired to 10 possible JMS priorities(0=>9). A mapping consists of a "|" separated list of value-to-range pairs (tuxvalue:jmsrange) where pairs are separated by ":" and ranges are separated by "-". Examples: 1:0 | 12:1 | 23:2 | 34:3 | 45:4 | 56:5 | 67:6 | 78:7 | 89:8 | 100:9 OR 20:0-1 | 40:2-3 | 60:4-5 | 80:6-7 | 100:8-9 MBean: weblogic.management. configuration. WTCtBridgeGlobalMBean Attribute: TuxToJmsPriorityMap | Readable: yes Writable: yes