bea.com | products | dev2dev | support | askBEA

Download Docs | Site Map | Glossary
Search

Administration Console Online Help

SNMP --> Traps --> Counter Monitor --> Configuration

Tasks Additional Documentation Attributes

Overview

Use this tab to configure Counter Monitors.

Tasks

Configuring a Counter Monitor

Additional Documentation

(Requires an Internet connection.)

WebLogic SNMP Management Guide

W ebLogic SNMP MIB Reference

Attributes

Attribute Label | Description | Value Constraints
--- | --- | ---
Name | The name of this configuration. WebLogic Server uses an MBean to implement and persist the configuration. MBean: weblogic.management. configuration. SNMPCounterMonitorMBean Attribute: Name | Configurable: yes Readable: yes Writable: yes
Monitored MBean Type | Defines the type of the MBean to monitor. MBean: weblogic.management. configuration. SNMPCounterMonitorMBean Attribute: MonitoredMBeanType | Configurable: yes Readable: yes Writable: yes
Monitored MBean Name | Defines the name of the MBean to monitor. MBean: weblogic.management. configuration. SNMPCounterMonitorMBean Attribute: MonitoredMBeanName | Configurable: yes Readable: yes Writable: yes
Monitored Attribute Name | Defines the name of an attribute to monitor. MBean: weblogic.management. configuration. SNMPCounterMonitorMBean Attribute: MonitoredAttributeName | Configurable: yes Readable: yes Writable: yes
Polling Interval | Defines the frequency the agent checks the attribute value. MBean: weblogic.management. configuration. SNMPCounterMonitorMBean Attribute: PollingInterval | Units: seconds Minimum: 0 Maximum: 65535 Default: 0 Configurable: yes Readable: yes Writable: yes
Threshold | Specifies a value that triggers the Counter Monitor to generate a trap. The Counter Monitor generates a trap each time it polls the value and determines that the value has transitioned from below the threshold to at or above the threshold. While the value remains at or above the threshold, the Counter Monitor does not generate additional traps. MBean: weblogic.management. configuration. SNMPCounterMonitorMBean Attribute: Threshold | Minimum: 0 Default: 0 Configurable: yes Readable: yes Writable: yes
Offset | Specifies an integer value to be added to the threshold if the threshold is crossed. For example, if you set Threshold to 1000 and Offset to 2000, when the observed attribute exceeds 1000, the Counter Monitor sends a notification and increases the threshold to 3000. When the observed attribute exceeds 3000, the Counter Monitor sends a notification and increases the threshold again to 5000. The threshold can increase up to a maximum specified by the Modulus attribute. MBean: weblogic.management. configuration. SNMPCounterMonitorMBean Attribute: Offset | Minimum: 0 Default: 0 Configurable: yes Readable: yes Writable: yes
Modulus | Specifies the maximum value for the threshold. You can specify an offset that causes the threshold to increase. When the threshold reaches the value specified by the Modulus, the threshold is returned to its original value before any offsets were applied. For example, if the original threshold is set to 1000 and the modulus is set to 5000, when the threshold exceeds 5000, the monitor sends a notification and resets the threshold to 1000. If you specify 0, the Counter Monitor does not use the modulus and the threshold value can grow indefinitely. MBean: weblogic.management. configuration. SNMPCounterMonitorMBean Attribute: Modulus | Minimum: 0 Default: 0 Configurable: yes Readable: yes Writable: yes