Skip navigation.
Downloads | Product Documentation | Support

Administration Console Online Help

# Local Tuxedo Access Points --> General

Tasks Related Topics Attributes

## Overview

Local Tuxedo Access Points provide configuration information to connect available remote Tuxedo domains to a WTC Service. You must have at least one Local Tuxedo Access Point configured to create a WTC Service.

## Tasks

Creating a Local Tuxedo Access Point

## Related Topics

Configuring WebLogic Tuxedo Connector

## Attributes

Table 423-1

Attribute Label | Description | Value Constraints
--- | --- | ---
Access Point | Defines a name used to identify a local Tuxedo access point in a WTC Service. This name must be unique within defined Local Tuxedo Access Points. This allows you to define unique configurations having the same Access Point ID. MBean: `weblogic.management. configuration. WTCLocalTuxDomMBean` Attribute: `AccessPoint` |
Access Point Id | The connection principal name used to identify this local Tuxedo access point when attempting to establish a session connection with a remote Tuxedo access point. The AccessPointId must match the corresponding DOMAINID in the *DM_REMOTE_DOMAINS section of your Tuxedo DMCONFIG file. MBean: `weblogic.management. configuration. WTCLocalTuxDomMBean` Attribute: `AccessPointId` |
Network Address | The network address and port number of this local Tuxedo access point. Specify the TCP/IP address in one of the following formats: `//hostname:port_number` `//#.#.#.#:port_number` If the hostname is used, the access point finds an address for hostname using the local name resolution facilities (usually DNS). If dotted decimal format is used, each # should be a number from 0 to 255. This dotted decimal number represents the IP address of the local machine. The port_number is the TCP port number at which the access point listens for incoming requests. MBean: `weblogic.management. configuration. WTCLocalTuxDomMBean` Attribute: `NWAddr` |