Skip navigation.
Downloads | Product Documentation | Support

Administration Console Online Help

# WTC Service --> Contents --> Local Access Points

Local Access Points (Local APs) provide configuration information to connect available remote Tuxedo domains to a WTC Service. You must have at least one Local Tuxedo Access Point configured to create a WTC Service.

- For information on how to create a Local Tuxedo Access Point, see Creating a Local Tuxedo Access Point.
- For information on how to configure network connections, see Configuring Connection Attributes for Local Tuxedo Access Points.
- For information on how to configure security attributes, see Configuring Security Attributes for Local Tuxedo Access Points.
- For information on how to delete a Local Tuxedo Access Point, see Deleting a Local Tuxedo Access Point.