Skip navigation.
Downloads | Product Documentation | Support

Administration Console Online Help

# Local Tuxedo Access Points: General

Configuration Options Related Tasks Related Topics

Use this page to define the general configuration of a local Tuxedo access point that will be used with this WTC Service.

#### Configuration Options

Name | Description
--- | ---
Access Point Name | The unique name used to identify this local Tuxedo access point. This name should be unique for all local and remote Tuxedo access points defined within a WTC Service. This allows you to define unique configurations having the same Access Point ID. MBean Attribute: `WTCLocalTuxDomMBean.AccessPoint`
Access Point ID | The connection principal name used to identify this local Tuxedo access point when attempting to establish a session connection with remote Tuxedo access points. Note: The AccessPointId must match the corresponding DOMAINID in the *DM_REMOTE_DOMAINS section of your Tuxedo DMCONFIG file. MBean Attribute: `WTCLocalTuxDomMBean.AccessPointId`
Network Address | The network address and port number of this local Tuxedo access point. Specify the TCP/IP address in the format: `//hostname:port_number` or `//#.#.#.#:port_number`. Note: If the hostname is used, the access point finds an address for hostname using the local name resolution facilities (usually DNS). If dotted decimal format is used, each # should be a number from 0 to 255. This dotted decimal number represents the IP address of the local machine. The port_number is the TCP port number at which the access point listens for incoming requests. MBean Attribute: `WTCLocalTuxDomMBean.NWAddr`

Related Tasks

- Create local access points
- Configure connections for local APs
- Configure security for local APs
- Delete local Tuxedo access points

Related Topics

- Configuring WebLogic Tuxedo Connector