Skip navigation.
Downloads | Product Documentation | Support

Socket Subsystem Messages The Socket1.0 catalog contains messages in the range BEA400 - BEA499. Messages in this catalog are part of the `weblogic.socket` Internationalization package and the `weblogic.i18n` Localization package.
BEA-000400 | Debug: msg
Description | Uncatalogued debug message - please do not change
Cause | Debugging - please do not change.
Action | No action required.
BEA-000401 | Critical: Socket queue full, dropping socket\n qfe.
Description | The internal queue for socket read requests is full. Additional read requests for sockets will be dropped.
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000402 | Warning: There are: numSockets active sockets, but the maximum number of socket reader threads allowed by the configuration is: getMaxSocketReaders. You may want to alter your configuration.
Description | A non-native IO is being used, and the number of socket reader threads is less than the number of active sockets. Performance may degrade significantly. It is recommended that you change the socket reader settings to improve the performance.
Cause | When non-native IO is used, IO is performed in a blocking manner. Therefore, if the number of socket reader threads is less than the number of active sockets, performance may degrade significantly.
Action | Increase ThreadPoolPercentSocketReaders and/or ThreadPoolSize, and/or decrease SocketReaderTimeoutMinMillis and/or SocketReaderTimeoutMaxMillis.
BEA-000403 | Error: IOException occurred on socket: socket\n ioe.
Description | An IO exception was encountered while reading from the socket.
Cause | An unexpected IO exception was encountered while performing IO for the socket.
Action | Check network connectivity. If situation persists after environmental issues are resolved, contact BEA Customer Support.
BEA-000404 | Critical: ThreadDeath in processSockets\n td.
Description | A ThreadDeath error was caught while processing sockets.
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000405 | Error: Uncaught Throwable in processSockets\n t.
Description | A Throwable was caught while processing sockets.
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000406 | Info: time_stamp
Cause | This is an informational message.
Action | No action required.
BEA-000407 | Warning: Cannot find getCPUCount() method\n bizzare.
Description | The native method getCPUCount() cannot be found.
Cause | Native implementation for getCPUCount method is not found.
Action | Make sure that the muxer shared library is in the correct library path. If situation persists, contact BEA Customer support.
BEA-000408(retired) | Info: Allocating nreaders NT reader threads
Cause | An informational message.
Action | No action required.
BEA-000409 | Error: Problem on socket: sock\n e
Description | An exception happened while registering the socket with the muxer.
Cause | An exception occurred while registering the socket with the muxer. It is possible that the file descriptor cannot be obtained from the socket.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000410(retired) | Warning: Attempt to read from socket sock that has been shutdown.
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000411(retired) | Warning: No IORecord present for fd: fd
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000412(retired) | Warning: No MuxableSocket present for fd: fd
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000413(retired) | Error: Failure in processSockets() - GetData: gd\n t
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000414 | Alert: Could not initialize POSIX Performance Pack.
Description | Could not load the shared library for the POSIX Performance Pack.
Cause | Unable to load the shared library for the POSIX Performance Pack.
Action | Make sure that the muxer shared library (libmuxer.so) exists in a directory that is in the LD_LIBRARY_PATH. If situation persists, contact BEA Customer Support.
BEA-000415 | Info: System has file descriptor limits of - soft: soft, hard: hard
Cause | An informational message.
Action | No Action Required.
BEA-000416 | Info: Using effective file descriptor limit of: current open sockets/files.
Cause | An informational message.
Action | No action required.
BEA-000417(retired) | Alert: Could not schedule trigger\n tte
Cause | Internal error: an attempt to schedule an internal trigger for the muxer failed.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000418(retired) | Info: Allocating: nreaders POSIX reader threads.
Cause | An informational message.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000419(retired) | Critical: Failure in timeout callback\n t.
Cause | Internal error: an failure occurred in socket timeout callback.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000420(retired) | Error: Bad result: polled from poll().
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000421 | Error: Uncaught Throwable in processSockets\n t.
Description | An unhandled Throwable was caught while processing sockets.
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000422(retired) | Warning: Got exception for fd: fd with no corresponding table entry
Cause | Internal Error.
Action | No action required.
BEA-000423(retired) | Warning: Got data for fd: fd with no corresponding table entry.
Cause | Internal Error.
Action | No action required.
BEA-000424(retired) | Error: IOException on socket: sock, fd: fd\n ioe.
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000425(retired) | Error: Got data for fd: fd but getSocket() returned null.
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000426(retired) | Info: SO_TIMEOUT was zero for: socket.
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000427(retired) | Error: Received interrupted reading from socket: socket fd: fd\n iioe.
Cause | Internal Error.
Action | No action required.
BEA-000428(retired) | Error: Unable to load performance pack, using Java I/O instead. msg\n t
BEA-000429 | Error: Muxer received error: msg\n t.
Description | An unexpected error was caught while processing sockets.
Cause | An unexpected error was encountered while processing socket IO requests.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000430 | Debug: msg\n e
Description | Uncatalogued debug message - please do not change.
Cause | Debugging - please do not change.
Action | No action required.
BEA-000431 | Info: Accepted Connection: Filtering is set to: "filterOn" Remote Address: "rAddr" Remote Port: "rPort" Local Address: "lAddr" Local Port: "lPort" Protocol: "protocol"
Description | Detailed information about an incoming connection.
Cause | Informational message for administrator.
Action | No action required.
BEA-000432 | Error: Unable to load performance pack. Using Java I/O instead.\n t
Description | Unable to load the native library for the performance pack. Using Java I/O instead.
Cause | Unable to load the native library for the performance pack.
Action | Make sure that the classpath and the environment is set up properly. If situation persists, contact BEA Customer Support.
BEA-000433(retired) | Error: Unable to load performance pack. Using Java I/O instead. msg\n t
Description | Unable to load the native performance pack. Using non-native Java I/O instead.
Cause | Unable to load the native performance pack.
Action | Make sure the appropriate path for the native libraries is set properly in the environment.
BEA-000434(retired) | Error: Unable to create Java Muxer.
Description | Creation of the Java socket muxer failed.
Cause | Internal Error.
Action | Make sure the classpath is set properly. If situation persists, contact BEA Customer Support.
BEA-000435 | Error: Unable to initiate read for the socket. The maximum allowed number of pending IO requests (maxfds) have exceeded.
Description | The maximum allowed number of pending IO requests (maxfds) have exceeded. Further read requests for socket cannot be initiated.
Cause | Internal Error.
Action | Contact BEA Customer Support. Please capture errors and send the server log files to support.
BEA-000436 | Info: Allocating nreaders reader threads.
Cause | An informational message.
Action | No action required.
BEA-000437 | Error: SSL is not supported when using nio. Please either disable native I/O, or use the standard performance pack.
Description | The NIO socket muxer does not support SSL. If SSL support is required, please either use non-native IO or the standard performance packs.
Cause | When using the NIO socket muxer, SSL is not supported.
Action | Either disable native I/O, or use the standard performance pack.
BEA-000438 | Error: Unable to load performance pack. Using Java I/O instead. msg\n
Description | Unable to load the native performance pack. Using non-native Java I/O instead.
Cause | Unable to load the native performance pack.
Action | Make sure the appropriate path for the native libraries is set properly in the environment.
BEA-000439 | Error: Unable to create Java Muxer.
Description | Creation of the Java socket muxer failed.
Cause | Internal Error.
Action | Make sure the classpath is set properly. If situation persists, contact BEA Customer Support.
BEA-000440 | Error: Unable to initiate IO for socket\n ex.
Description | Initiation of the IO operation failed.
Cause | The initiation of the IO operation failed, which could be caused by network, IO or other problems. It could also be an internal error.
Action | Correct any conditions as suggested by the error message if applicable. If situation persists, contact BEA Customer Support.
BEA-000441 | Warning: Unable to find internal data record for the socket socket, with IO completion result success
Description | Unable to find internal data record for the socket while completing an IO operation.
Cause | Internal Error.
Action | If situation persists, contact BEA Customer Support.
BEA-000442 | Warning: Connection attempt was rejected because the incoming protocol is not enabled on channel "channel".
Description | The Connection attempt was rejected because a protocol is not enabled on this channel or Listen Address.
Cause | The Connection attempt was rejected because a protocol is not enabled at all for this server, as determined by the ServerMBean, or is not enabled on this particular channel.
Action | Enable the protocol on the channel.
BEA-000443 | Warning: Connection attempt was rejected because the incoming protocol protocol is not enabled on channel channel.
Description | The Connection attempt was rejected because the protocol protocol is not enabled on this channel or Listen Address.
Cause | The Connection attempt was rejected because the protocol protocol is not enabled at all for this server, as determined by the ServerMBean, or is not enabled on this particular channel.
Action | Enable the protocol protocol on the channel.
BEA-000444 | Warning: Could not load the performance pack that can take advantage of /dev/(e)poll device due to:\n\tt. \nWill attempt to use the performance pack that does not depend on /dev/(e)poll device.
Description | Could not load the performance pack that can take advantage of /dev/(e)poll device due to:\n\tt. \nWill attempt to use the performance pack that does not depend on /dev/(e)poll device.
Cause | Your OS does not support /dev/(e)poll or the device is not initialized.
Action | Ensure that your OS supports the /dev/(e)poll device.
BEA-000445 | Notice: Connection rejected, filter blocked sock0, fe1
Description | The incoming message was not recognised as one of the supported protocols
Cause | The incoming message was not recognised as one of the supported protocols
Action | Ensure that the server is configured for the relevant protocol
BEA-000446 | Info: Native IO Enabled.
Cause | This is an informational message.
Action | No action required.
BEA-000447 | Info: Native IO Disabled. Using Java IO.
Cause | This is an informational message.
Action | No action required.