Overview | Namespace | Component | Index | Help
| BEA WebLogic Server 9.1 Domain Configuration Schema Reference
DETAILS: DOCUMENTATION | ELEMENTS | ATTRIBUTES | FRAMES | NO FRAMES

## http://www.bea.com/ns/weblogic/90/domain
element nw-addr

Model
  `<nw-addr>string</nw-addr>`

Disallowed substitutions (block)
  none (extensions, restrictions and substitutions are allowed)

Substitution group exclusion (final)
  none (extensions and restrictions are allowed)

Usage

Documentation

  The network address and port number of this remote Tuxedo access point. Specify the TCP/IP address in the format: `//hostname:port_number` or `//#.#.#.#:port_number`.

  Note: If the hostname is used, the access point finds an address for hostname using the local name resolution facilities (usually DNS). If dotted decimal format is used, each # should be a number from 0 to 255. This dotted decimal number represents the IP address of the local machine. The port_number is the TCP port number at which the access point listens for incoming requests.

  Privileges: Read/Write

  Default Value: //localhost:8902

  MBean Attribute: `WTCRemoteTuxDomMBean.NWAddr`

Fundamental Facets
  equality, non-numeric, unbounded, unordered, countable infinite value space

White Space Processing
  collapse

Overview | Namespace | Component | Index | Help
| BEA WebLogic Server 9.1 Domain Configuration Schema Reference
DETAILS: DOCUMENTATION | ELEMENTS | ATTRIBUTES | FRAMES | NO FRAMES

Version: 9.1