Overview | Namespace | Component | Index | Help
| BEA WebLogic Server 9.1 Domain Configuration Schema Reference
DETAILS: DOCUMENTATION | ELEMENTS | ATTRIBUTES | FRAMES | NO FRAMES

## http://www.bea.com/ns/weblogic/90/domain
element cmp-limit

Model
  `<cmp-limit>annonymous type derived from int</cmp-limit>`

Disallowed substitutions (block)
  none (extensions, restrictions and substitutions are allowed)

Substitution group exclusion (final)
  none (extensions and restrictions are allowed)

Usage

Documentation

  The compression threshold this remote Tuxedo access point uses when sending data to a local Tuxedo access point. Application buffers larger than this size are compressed.

  Range of Values: Between `0` and a positive 32-bit integer.

  Privileges: Read/Write

  Default Value: 2147483647

  Minimum value: `0`

  Maximum value: `2147483647`

  MBean Attribute: `WTCRemoteTuxDomMBean.CmpLimit`

Fundamental Facets
  equality, numeric, bounded, totaly ordered, countable infinite value space

White Space Processing
  collapse

Pattern Facet
  `[\-+]?[0-9]+`

Digits Facets
  fraction digits: 0

Overview | Namespace | Component | Index | Help
| BEA WebLogic Server 9.1 Domain Configuration Schema Reference
DETAILS: DOCUMENTATION | ELEMENTS | ATTRIBUTES | FRAMES | NO FRAMES

Version: 9.1