Previous Next JavaScript must be enabled to correctly display this content

## 2 Configuration

This topic describes the systematic instructions to perform the configuration.

End-user can configure the properties w.r.t. monitoring, alert and export.

End-user can configure the same at System level and granular levels such as Consumer, Consumer Service and Routing.

The Configuration screen contains the following sections.

- Monitoring - It has the features required by the breaker to store and aggregate the result of calls.
- Alert - It has the features required for transitioning circuit breaker.
- Email Alert - It has the feature required for mail notification.
- Export - It has the properties that are required for exporting the configuration JSON and will be visible at system level only.

Specify User ID and Password, and login to Home screen.

1. On Home screen, click Core Maintenance. Under Core Maintenance, click Routing Hub.
2. Under Routing Hub, click Configuration.
   The Configuration screen displays.

   Figure 2-1 Configuration

   Description of "Figure 2-1 Configuration"
3. Specify the fields on Configuration screen.

   Note:

   The fields, which are marked with an asterisk, are mandatory.
   For more information on fields, refer to the field description table.

   Table 2-1 Configuration - Field Description

   Field | Description
   --- | ---
   Window Type | Select the type of the window. The available options are: Count: The count-based sliding window aggregates the outcome of the last N calls (Window Size). Time: The time-based sliding window aggregates the outcome of the calls of the last N seconds (Window Size).
   Window Size | Specify the window size to record the outcome of the calls when the circuit breaker is closed. For Count window type, The window size is N calls. For Time window type, The window size has N seconds.
   Minimum number of calls | Specify the minimum number of calls. For example: If the minimum number of calls are 10, then at least 10 calls must be recorded before calculating the failure rate. If only nine calls are recorded, the circuit breaker is not transitioned to open even if all nine calls are failed.
   Failure rate threshold | Specify the failure rate threshold in percentage. When the failure rate is equal or greater than the threshold, the circuit breaker transitions to open and starts short-circuiting calls.
   Email Addresses | Specify the E-mail address. The user can use semi-colon to add more email addresses. Once the failure rate crosses the Failure rate threshold, a mail is sent to the end-user about the event.
   Mark data as factory shipped | Select the toggle to mark the exported configuration JSON as factory shipped JSON. The end-user will not be able to modify or delete the certain data once imported. By default, the toggle is OFF.

   Example:

   Table 2-2 Configuration - Field Entry Values

   Field | Entry Values
   --- | ---
   Window Type | Count
   Window Size | 20
   Minimum number of calls | 10
   Failure rate Threshold | 50%

   Configured properties will result as below:

   After 10 (minimum number of calls) calls, routing would get shutdown if 50% (failure rate) of almost last 20 (window size) calls have failed. If the email address property is configured, then the end-user is notified as well.

4. Click Clear to clear all the specified details.
5. Click Reset to reset the details.
6. Click Save to save all the details.