bea.com | products | dev2dev | support | askBEA

Download Docs | Site Map | Glossary
Search

Administration Console Online Help

SNMP --> Proxies --> General

Tasks Additional Documentation Attributes

Overview

Use the this tab to configure a proxy.

Tasks

Configuring an SNMP Proxy

Additional Documentation

(Requires an Internet connection.)

WebLogic SNMP Management Guide

W ebLogic SNMP MIB Reference

Attributes

Attribute Label | Description | Value Constraints
--- | --- | ---
Name | The name of this configuration. WebLogic Server uses an MBean to implement and persist the configuration. MBean: weblogic.management. configuration. SNMPProxyMBean Attribute: Name | Configurable: yes Readable: yes Writable: yes
Port | Defines the Port number used for communication with the other SNMP Agents. MBean: weblogic.management. configuration. SNMPProxyMBean Attribute: Port | Minimum: 0 Maximum: 65535 Default: 0 Configurable: yes Readable: yes Writable: yes
Oid Root | Defines the root of the OID tree on which the proxied agent responds. MBean: weblogic.management. configuration. SNMPProxyMBean Attribute: OidRoot | Configurable: yes Readable: yes Writable: yes
Community | Defines the community name to be passed on for all requests to the proxied agent. Default value is the community name contained in incoming SNMP requests to the Master SNMP agent. MBean: weblogic.management. configuration. SNMPProxyMBean Attribute: Community | Default: "na" Configurable: yes Readable: yes Writable: yes
Timeout | Defines the time interval that the WebLogic SNMP proxy agent waits for a response to requests forwarded to another SNMP agent. If the interval elapses without a response, the WebLogic SNMP agent sends an error to the requesting manager. MBean: weblogic.management. configuration. SNMPProxyMBean Attribute: Timeout | Units: milliseconds Minimum: 0 Default: 5000 Configurable: yes Readable: yes Writable: yes