Overview | Namespace | Component | Index | Help
| BEA WebLogic Server 9.1 Domain Configuration Schema Reference
DETAILS: DOCUMENTATION | ELEMENTS | ATTRIBUTES | FRAMES | NO FRAMES

## http://www.bea.com/ns/weblogic/90/domain
element tunneling-client-ping-secs

Model
  `<tunneling-client-ping-secs>annonymous type derived from int</tunneling-client-ping-secs>`

Disallowed substitutions (block)
  none (extensions, restrictions and substitutions are allowed)

Substitution group exclusion (final)
  none (extensions and restrictions are allowed)

Usage

Documentation

  The interval (in seconds) at which this network channel should ping an HTTP-tunneled client to see if its still alive. A value of `-1` indicates that the network channel obtains this interval from the ServerMBean. (Requires you to enable tunneling for the network channel.)

  Privileges: Read/Write

  Minimum value: `1`

  MBean Attribute: `NetworkAccessPointMBean.TunnelingClientPingSecs`

Fundamental Facets
  equality, numeric, bounded, totaly ordered, countable infinite value space

White Space Processing
  collapse

Pattern Facet
  `[\-+]?[0-9]+`

Digits Facets
  fraction digits: 0

Overview | Namespace | Component | Index | Help
| BEA WebLogic Server 9.1 Domain Configuration Schema Reference
DETAILS: DOCUMENTATION | ELEMENTS | ATTRIBUTES | FRAMES | NO FRAMES

Version: 9.1